***This text should be copied and pasted to appropriate section of Division 04 project specifications.***

***Important! The specification of the CavClear products affects details as well. CAD specialist should contact CavClear/Archovations for information.***

**PART 1 – GENERAL**

1. SUMMARY
   1. Weep vents.
2. SUBMITALS
   1. Submit two samples weep vents, actual size and color, and manufacturer's product datasheet.
3. DELIVERY, STORAGE AND HANDLING
   1. Protect weep vents packaging from rain.

**PART 2 – PRODUCTS**

1. WEEP VENTS
   1. Manufacturer and Type: CavClear Weep Vents as manufactured by Archovations, Inc., 701 Second Street, Hudson, WI 54016, (715) 381-5773.
      1. Description: Non-woven mesh with M-notched bottom.
      2. Color [selected by Project Architect] [manila] [harvest gold] [gray] to match mortar.
      3. Size: 3/8 inch by [2-1/2 inches high by 3-1/2 inches] [\_\_\_\_\_\_\_\_\_\_\_\_\_] wide.

**PART 3 – EXECUTION**

1. INSTALLATION
   1. Place weep vents in head joints at exterior wythe of cavity wall located immediately above ledges and flashing, spaced 24 inches on center, unless otherwise shown. Leave the side of the masonry units forming the vent space unbuttered and clear of mortar. Install with notched side down. Slide vent material into joint as the two masonry units forming the weep vent are placed.